HW 4

Josh Pradera

A user space driver doesn’t require a kernel module since the memory mapping allows user space to map to the Ethernet controller hardware registers directly

bypassing the need for a kernel module.